ip nat inside source static? 192.168.10.254 <inside local> 209.165.201.5 <inside global>
ip nat? <inside> or <outside> at config-if#


?// clear stats before testing
clear ip nat statistics? at config# 

?Steps for dynamic NAT config
?// 1. config dynamic pool on edge router 
ip nat pool NAT-POOL1? 209.165.200.226 209.165.200.240 netmask 255.255.255.224 at config#
?// 2. create acl to permit users
access-list 1 permit? 192.168.0.0 0.0.255.255 at config#
?// 3. bind acl to pool adds
ip nat inside source list 1 pool NAT-POOL1? at config#
?// 4. config inside int
int? s0/1/0
ip nat inside?? at config-if#
?// 5. config outside int
int? s0/1/1
ip nat outside? ? at config-if#

clear ip nat trans *? at config#


show ip nat translations
show ip nat trans verbose
show ip nat statistics
show running-config | include NAT








