config t
username admin privilege 15 secret ?password12345
line vty ?0 4
transport input ?ssh
login local
exit
crypto key generate rsa general-keys
1024
yes

ip ssh time-out ?75
ip ssh authentication-retries ?2

exit
end
copy running-config startup-config
wr

show ip int brief
show ip ssh
show interface ?fa0/1