config t
access-list 10 remark ?Allow traffic R1
access-list 10 permit ?192.168.0.0 0.0.31.255
access-list 10 permit host ?192.168.0.1
access-list 10 deny ?192.168.0.0
access-list 10 deny any
access-list end

Ip access-list standard ?SOME-POLICY or 10
remark ?ACL Policy for Something-in
permit ?192.168.0.10 0.0.31.255(wildcard)
permit host ?192.168.0.5
deny ?2.2.2.2 0.0.0.0
40 permit ?192.168.10.0 0.0.0.255(add to list)
deny any
end

interface ?fa0/1
ip access-group ?10 out
ip access-group ?SOME-POLICY in

exit
end
copy running-config startup-config
wr

show access-lists
show ip access-lists
show access-list ?10
show ip int ?fa0/1