enable
config t
hostname ?R1
no ip domain-name 
ip domain-name ?example.com
security passwords min-length ?10
enable secret ?password10
line console ?0
password ?otherpswd
exec-timeout ?75
login 
logging synchronous 
line vty ?0 15
service password encryption 
banner MOTD # ?Unauthorized access is strictly prohibited. #

exit 
end 
copy running-config startup-config
wr

show ip route
show ip int brief
show ip int ?fa0/1
show running-config
